The use case 3, calibrate room boundaries, is changed because we misunderstood the concept and almost describe it same as a combined version of other cases(When user enters a new room, the server decides if to connect to that speaker).

For Use Case #5, 3A and 3B have been combined into a single alternate flow. They are very similar problems and have the exact same procedure.

For Use Case #7, the alternate flows have been modified so that 1B and 1C have been removed. They were redundant cases.

For Use Case #10, the wording for the alternate flow was made more concise.