The use case 3, calibrate room boundaries, is changed because we misunderstood the concept and almost describe it same as a combined version of other cases(When user enters a new room, the server decides if to connect to that speaker).